IZOROL-SR EPS 200 and IZOROL-SR/KL EPS 200 
1. Description 
Insulation boards Izorol-SR are made of styrofoam EPS 200  coated on one side with polypropylene fabric  coated with polypropylene . Standard dimensions : length 200 cm, width 100 cm ( packed 10 boards dimensions 100cm X 200 cm) thickness 10mm, 12mm or 15mm. 
Insulation boards Izorol-SR/KL are made of styrofoam EPS 200 coated on one side with polypropylene fabric  coated with polypropylene and an additional bottom layer of glue with a transparent siliconized foil. The transparent siliconized foil protects the bottom layer of the product during transport. The glue used in the bottom layer is used to fix the board to the surface.  Insulation board standard dimensions : length 100 cm, width 100 cm 
( packed 20 boards dimensions  100cm X 100 cm) thickness 10mm, 12mm or 15mm. 
2. Application 
The boards are used as thermal, acoustic and damp insulation in water floor heating systems in residential building as well as public utilities. The main advantage of Izorol-SR and Izorol-SR/KL boards is their top endurance of the surface (fabric) to tearing. It is of great importance in case of single-layer pipes requiring stronger anchoring in insulation. 


IZOROL-SR EPS T and IZOROL-SR/KL EPS T 
1. Description
Insulation boards Izorol-SR  EPS T are made of styrofoam EPS T coated on one side with polypropylene fabric  coated with polypropylene . Standard dimensions : length 200 cm, width 100 cm (packed 10 boards dimensions 100cm X 200 cm) thickness 10mm, 12mm or 15mm. 
Insulation boards Izorol-SR/KL are made of styrofoam EPS T coated on one side with polypropylene fabric  coated with polypropylene and an additional bottom layer of glue with a transparent  siliconized foil. The transparent siliconized foil protects the bottom layer of the product during transport. The glue used in the bottom layer is used to fix the board to the surface.  Insulation board standard dimensions : length 100 cm, width 100 cm (packed 20 boards  dimensions 100cm X 200 cm) thickness 10mm, 12mm or 15mm. 
2. Application 
The boards are used as thermal, acoustic and damp insulation in water floor heating systems in residential building as well as public utilities. The main advantage of Izorol-SR and Izorol-SR/KL boards is their top endurance of the surface (fabric) to tearing. It is of great importance in case of single-layer pipes requiring stronger anchoring in insulation. 



WELDED CLAMPS FOR ATTACHING UNDERFLOOR HEATING PIPES IN LOADES TO THE TACKER
1. Description 
Tube clamps welded in stapler loads for floor heating pipes are made of polypropylene coloured: red, blue or black. Clamps come in stapler loads -20 loads of 30 clamps. Collective packaging consists of 20 boxes, each  of 600 pieces,  which the total 12000 pieces.
Welded clamps dimensions:
Length: 30mm
Thickness max. :9,1 mm
Width :35 mm
Maximum pipe’s diameter :17 mm

2. Application
Welded clamps are used to fasten underfloor heating pipes with maximum diameter 17 mm to insulation boards with a minimum thickness of 10 mm. 






